<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="18.278" y1="-1.312" x2="61.979" y2="-1.312" width="0" layer="20"/>
<wire x1="61.979" y1="-1.312" x2="61.979" y2="20.589" width="0" layer="20"/>
<wire x1="61.979" y1="20.589" x2="18.278" y2="20.639" width="0" layer="20"/>
<wire x1="18.278" y1="20.639" x2="18.278" y2="-1.312" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="analog-devices">
<packages>
<package name="SO8">
<description>&lt;b&gt;8-Lead Small Outline IC&lt;/b&gt; (SO-8)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf</description>
</package>
</packages>
</library>
<library name="con-molex">
<packages>
<package name="53047-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X15">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R_F4" library="SparkFun-Passives" package="0603-RES" value="1k43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_F1" library="SparkFun-Passives" package="0603-RES" value="1k43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_F2" library="SparkFun-Passives" package="0603-RES" value="1k43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R_F3" library="SparkFun-Passives" package="0603-RES" value="1k43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C_F4" library="SparkFun-Capacitors" package="0402-CAP" value="220nF">
<attribute name="PROD_ID" value="CAP-09885"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C_F1" library="SparkFun-Capacitors" package="0402-CAP" value="220nF">
<attribute name="PROD_ID" value="CAP-09885"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C_F3" library="SparkFun-Capacitors" package="0402-CAP" value="220nF">
<attribute name="PROD_ID" value="CAP-09885"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C_F2" library="SparkFun-Capacitors" package="0402-CAP" value="220nF">
<attribute name="PROD_ID" value="CAP-09885"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C_P" library="SparkFun-Capacitors" package="0402-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0402-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0402-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0402-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0402-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RG1" library="SparkFun-Passives" package="0603-RES" value="450">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RG2" library="SparkFun-Passives" package="0603-RES" value="450">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RG3" library="SparkFun-Passives" package="0603-RES" value="450">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RG4" library="SparkFun-Passives" package="0603-RES" value="450">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A1" library="analog-devices" package="SO8" value="">
<attribute name="OC_NEWARK" value="05F7109"/>
<attribute name="MPN" value="AD620AR"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1464424"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A2" library="analog-devices" package="SO8" value="">
<attribute name="OC_NEWARK" value="05F7109"/>
<attribute name="MPN" value="AD620AR"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1464424"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A3" library="analog-devices" package="SO8" value="">
<attribute name="OC_NEWARK" value="05F7109"/>
<attribute name="MPN" value="AD620AR"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1464424"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A4" library="analog-devices" package="SO8" value="">
<attribute name="OC_NEWARK" value="05F7109"/>
<attribute name="MPN" value="AD620AR"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1464424"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LC1P" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LC1O" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LC2P" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LC2O" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LC3P" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LC3O" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LC4P" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LC4O" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SHD" library="SparkFun-Connectors" package="1X15" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A" library="SparkFun-Connectors" package="1X15" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="RG1" pad="2"/>
<contactref element="A1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="A1" pad="3"/>
<contactref element="LC1O" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="RG1" pad="1"/>
<contactref element="A1" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="A2" pad="3"/>
<contactref element="LC2O" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="RG2" pad="2"/>
<contactref element="A2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="RG2" pad="1"/>
<contactref element="A2" pad="8"/>
</signal>
<signal name="N$8">
<contactref element="A2" pad="2"/>
<contactref element="LC2O" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="RG3" pad="2"/>
<contactref element="A3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="RG3" pad="1"/>
<contactref element="A3" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="A3" pad="2"/>
<contactref element="LC3O" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="A4" pad="3"/>
<contactref element="LC4O" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="RG4" pad="2"/>
<contactref element="A4" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="RG4" pad="1"/>
<contactref element="A4" pad="8"/>
</signal>
<signal name="N$16">
<contactref element="A4" pad="2"/>
<contactref element="LC4O" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R_F1" pad="2"/>
<contactref element="A1" pad="6"/>
</signal>
<signal name="N$18">
<contactref element="R_F2" pad="2"/>
<contactref element="A2" pad="6"/>
</signal>
<signal name="N$19">
<contactref element="R_F3" pad="2"/>
<contactref element="A3" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="R_F4" pad="2"/>
<contactref element="A4" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="C_P" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="A1" pad="7"/>
<contactref element="A2" pad="7"/>
<contactref element="A3" pad="7"/>
<contactref element="A4" pad="7"/>
<contactref element="LC1P" pad="1"/>
<contactref element="LC2P" pad="1"/>
<contactref element="LC3P" pad="1"/>
<contactref element="LC4P" pad="1"/>
<contactref element="A" pad="12"/>
</signal>
<signal name="N$23">
<contactref element="R_F1" pad="1"/>
<contactref element="C_F1" pad="2"/>
<contactref element="A" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="A1" pad="2"/>
<contactref element="LC1O" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="C_F4" pad="1"/>
<contactref element="R_F4" pad="1"/>
<contactref element="A" pad="11"/>
</signal>
<signal name="N$22">
<contactref element="R_F3" pad="1"/>
<contactref element="C_F3" pad="2"/>
<contactref element="A" pad="10"/>
</signal>
<signal name="N$25">
<contactref element="R_F2" pad="1"/>
<contactref element="C_F2" pad="2"/>
<contactref element="A" pad="9"/>
</signal>
<signal name="GND">
<contactref element="C_F4" pad="2"/>
<contactref element="C_F3" pad="1"/>
<contactref element="C_F2" pad="1"/>
<contactref element="C_F1" pad="1"/>
<contactref element="C_P" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="A1" pad="4"/>
<contactref element="A1" pad="5"/>
<contactref element="A2" pad="4"/>
<contactref element="A2" pad="5"/>
<contactref element="A3" pad="4"/>
<contactref element="A3" pad="5"/>
<contactref element="A4" pad="4"/>
<contactref element="A4" pad="5"/>
<contactref element="LC1P" pad="2"/>
<contactref element="LC2P" pad="2"/>
<contactref element="LC3P" pad="2"/>
<contactref element="LC4P" pad="2"/>
<contactref element="A" pad="14"/>
</signal>
<signal name="N$9">
<contactref element="LC3O" pad="1"/>
<contactref element="A3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
