Dados das rodas da Harbor freight:

DIAMETER: 8-3/4" - 222.25mm  
CIRCUMFERENCE: 27-1/2" - 698.5 mm  
WIDTH: 2-3/8" - 60.324999999999996 mm  
RIM DIA.: 4" - 101.6mm  
AXLE DIA.: 5/8" - 15.875mm  
TIRE/TUBE SIZE: 2.50 - 4  
CONSTRUCTION: 4-PLY RATED 2-PLY  
MAXIMUM PRESSURE: 30 P.S.I.  
RIM BOLTS: 8MM  
BOLT HOLES: 9MM  
WEIGHT CAPACITY: 275 LBS.  
RECOMMENDED GREASE FITTINGS: NO  
APPLICATION: FOR LOW SPEED USE ONLY