Dados das rodas da Harbor freight:

DIAMETER: 8-3/4" - 222.25mm
CIRCUMFERENCE: 27-1/2" - 698.5 mm
WIDTH: 2-3/8" - 60.324999999999996 mm
RIM DIA.: 4" - 101.6mm
AXLE DIA.: 5/8" - 15.875mm
TIRE/TUBE SIZE: 2.50 - 4
CONSTRUCTION: 4-PLY RATED 2-PLY
MAXIMUM PRESSURE: 30 P.S.I.
RIM BOLTS: 8MM
BOLT HOLES: 9MM
WEIGHT CAPACITY: 275 LBS.
RECOMMENDED GREASE FITTINGS: NO
APPLICATION: FOR LOW SPEED USE ONLY